TopoScout - Sample CAD Files (SG-ZMVCSP)
=========================================

FILES:
  TopoScout_SG-ZMVCSP.dxf  - site drawing (State Plane, 45 layers)
  aerial_far.png           - wide aerial
  aerial_near.png          - close aerial

TO PLACE THE AERIALS (insert, then align):
  1. Open the DXF in your CAD software.
  2. Insert each image (far and near).
  3. Run the ALIGN command.
  4. Snap the image frame to the tick marks already
     placed in the drawing - it locks into position
     over your linework.

Questions? info@toposcout.com
